Strona wtórna:

1103 Measurement: Full Scale Voltage (100%) 220,0 kV 
1104 Measurement: Full Scale Current (100%) 1200 A 
1105 Line Angle 80 ° 
1211 Angle of inclination, distance charact. 85 ° 
1111 Line Length 96,5 km 
1116 Zero seq. comp. factor RE/RL for Z1 1,38 
1117 Zero seq. comp. factor XE/XL for Z1 0,40 
1118 Zero seq. comp.factor RE/RL(> Z1) 1,38 
1119 Zero seq. comp.factor XE/XL(> Z1) 0,40
1301 Operating mode Z1 Forward 
1302 R(Z1), Resistance for ph-ph-faults 15,000 Ohm 
1303 X(Z1), Reactance 18,580 Ohm 
1304 RE(Z1), Resistance for ph-e faults 22,000 Ohm

1351 Operating mode Z1B (overrreach zone) Forward 
1352 R(Z1B), Resistance for ph-ph-faults 15,000 Ohm 
1353 X(Z1B), Reactance 25,000 Ohm 
1354 RE(Z1B), Resistance for ph-e faults 22,000 Ohm 

1312 R(Z2), Resistance for ph-ph-faults 18,000 Ohm 
1313 X(Z2), Reactance 27,820 Ohm 
1314 RE(Z2), Resistance for ph-e faults 24,000 Ohm

1321 Operating mode Z3 Forward 
1322 R(Z3), Resistance for ph-ph-faults 20,000 Ohm 
1323 X(Z3), Reactance 43,090 Ohm 
1324 RE(Z3), Resistance for ph-e faults 26,000 Ohm

1331 Operating mode Z4 Forward 
1332 R(Z4), Resistance for ph-ph-faults 20,000 Ohm 
1333 X(Z4), Reactance 81,820 Ohm 
1334 RE(Z4), Resistance for ph-e faults 26,000 Ohm