

Wartości wtórne:
X1 =14,85 Ω                  R1ff=7,43		R1fe=15,62
X1w =20,09 Ω	              R1wff=8,13                 R1wfe=16,31
X2 =20,09 Ω                  R2ff=8,13                     R2fe=16,31
X3 =60,00 Ω                  R3ff=13,45                  R3fe=21,64

Measurement: Full Scale Voltage (100%) 220,0 kV 
Measurement: Full Scale Current (100%) 1200 A 
Line Angle 82 ° 
Angle of inclination, distance charact. 82 ° 
Line Reactance per length unit 0,2290 Ohm / km 
Line Length 76,3 km 
Zero seq. comp. factor RE/RL for Z1 1,60 
Zero seq. comp. factor XE/XL for Z1 0,40 
Zero seq. comp.factor RE/RL(> Z1) 1,60 
Zero seq. comp.factor XE/XL(> Z1) 0,40 